DY25/DY35 Small Wheel Loader

|  |  |
| --- | --- |
| **Model** | **DY25** |
| Dimensions: | 3615\*930\*2192mm |
| Operating Weight (Without Attachment) | 1360kgs |
| Max Travel Speed | 12km/h |
| Rated Operating Capacity(Bucket/Fork) | 809kg/527kg |
| Max.Dump Height | 3400mm |
| Tipping Height | 1970mm |
| Wheel Base | 1345mm |
| Turn Radius (Inside) | 865mm |
| Turn Radius (Outside) | 2210mm |
| Max. Turn Radius | 1829mm |
| Bucket Capacity | 0.3-0.48m3 |
| Working Oil Flow | 35L/Min |
| Tracking Oil Flow | 90L/Min |
| Tires | 27X8.5-15, 8PLY |
| **Engine Brand** | **Yanmar 3TNV76** |
| **Cooling System** | Water cooling |
| **Cylinders** | 3 Cylinders |
| **Engine Rated Power/R.P.M.** | 18.7KW (25H.P)/3200 r/min |

|  |  |
| --- | --- |
| **Model** | **DY35** |
| Dimensions: | 4140\*1090\*2260mm |
| Operating Weight (Without Attachment) | 2200kg |
| Max Travel Speed | 20km/h |
| Rated Operating Capacity(Bucket/Fork) | 1158kg/850kg |
| Max.Dump Height | 3717mm |
| Tipping Height | 2272mm |
| Wheel Base | 1502mm |
| Turn Radius (Inside) | 1106mm |
| Turn Radius (Outside) | 2625mm |
| Max. Turn Radius | 2206mm |
| Bucket Capacity | 0.3-0.48m3 |
| Working Oil Flow | 51L/Min |
| Tracking Oil Flow | 84L/Min |
| Tires | 27X10.5-15, 8PLY |
| Engine Brand/Model | Yanmar 3TNV88 |
| Cooling system | Water Cooling |
| Cylinders | 3 Cylinders |
| Rated Power/R.P.M. | 26.9KW/3000r/min |