**DY1150 Optional Engines**



|  |  |  |
| --- | --- | --- |
| **Engine brand** | **Yanmar 4TNV94L** | **KOHLER** KDI1903TCR |
| **Standard** | EURO III A | Terminal EPA Tier 4 |
| **Cooling System** | Water Cooling | Water Cooling |
| **Cylinders** | 4 Cylinders | 4 Cylinders |
| **Rotation Speed** | 2400 r/min | 2600 r/min |
| **Rated Power** | 35.5KW (48HP) | 42KW (57HP) |

**DY1150 Specifications**

|  |  |
| --- | --- |
| ****Model**** | ****DY1150**** |
| ****Dimension (LxWxH)**** | 3410mm\*1510mm\*2320mm |
| Max. reach(boom extended) | 3530mm |
| Max. reach(boom retracted) | 2908mm |
| Bucket capacity | 600L |
| Rated loading capacity | 1600kg |
| Tipping load | 2600kg |
| Min. turning radius | 1535mm |
| Ground clearance | 330mm |
| Turning angle | 45 Degree |
| Speed | 16.5 km/h |
| Weight | 2300 kg |
| Standard tire | 31X15.5-15 |
| Tire pressure | 2.8 bar |
| Oil tank capacity | 70L |
| Pressure | 200bar |
| Working oil flow | 82L/min |
| Tracking oil flow | 117L/min |
| Oil model(mineral oil) | L-HL46 |
| Fuel tank capacity | 32L |
| Battery capacity | 70Ah |
| Voltage | 12v |