**TL1500 Optional Engines**



****

|  |  |  |
| --- | --- | --- |
| **Engine Model** | **Yunnei YN27** | **Kohler KDI1903TCR** |
| **Engine power** | **58KW(79HP)** | 42KW(56HP) |
| **Rated Speed** | 2400 r/p.min | 2600 r/p.min |
| **Engine cooling way** | Water cooling | Water cooling |
| **Number of Cylinders** | 3 | 3 |
| **Engine type** | 4 cycle diesel Engine | 4 cycle diesel Engine |
| **Emission Standard** | Chinese II | **EPA Tier 4** |

**TL1500 Specifications**

|  |
| --- |
| **TL1500 Specifications** |
| **Overall Dimensions** | Overall Length | 4450mm |
| Overall Height | 2730mm |
| Overall Width | 1900mm |
| **Brake System** | Service Brake | Four Wheel Disk Brake |
| Parking Brake | Hand Operate |
| Braking Type | Air Braking |
| Axle | With hub reducer |
| **Tire Model** | 20.5-16, 12ply |
| **Max. Lifting Height** | 4500mm |
| **Max. Height to the Pin** | 4200mm |
| **Rated Load** | 1500kgs -1800kgs |
| **Max. Speed** | 17km/h |
| **Transmission System** | Hydraulic Converter+Drive Shaft+Axles |
| **Wheelbase** | 2430mm |
| **Min Turning Radius** | 4970mm |
| **Wheel Track** | 1345mm |
| **Weight** | 4360kg |
| **System Pressure** | 20Mpa |
| **Working Hydraulic Oil Flow** | 104L/min |
| **Walking Hydraulic Oil Flow** | 48L/min |

**TL1500 Specifications**