**TL2500 Optional Engines**

****

|  |
| --- |
| **TL2500 Optional Chinese Engines** |
| Engine Model | **YUNNEI** YN38GBZ | **YUNNEI YN4BL105-30CR** |
| Emission Standard | **Chinese II** | **Chinese III** |
| Engine Power | 76KW (103HP) | 77KW (105HP) |
| Rated Speed | 2400 r/p.min | 2400 r/p.min |
| Engine Cooling Way | Water cooling | Water cooling |
| Engine Type | 4 cycle diesel | 4 cycle diesel |

****

****

|  |
| --- |
| **TL2500 Optional EU or EPA Stage Engines** |
| **Engine Model** | **Xinchai 4E30YG52** | **Cummins QSF2.8** |
| Emission Standard | **Euro V** | **EPA Tier 4 / Euro III** |
| Engine Power | 55.8KW (76HP) | 55KW (75HP) |
| Rated Speed | 2200 r/p.min | 2500 r/p.min |
| Engine Cooling Way | Water cooling | Water cooling |
| Engine Type | 4 cycle diesel Engine | 4 cycle diesel Engine |

**TL2500 Specifications**

|  |
| --- |
| **TL2500 Specifications** |
| **Overall Dimensions** | Overall Length | 5000mm |
| Overall Height | 2860mm |
| Overall Width | 1950mm |
| **Brake System** | Service Brake | Four Wheel Disk Brake |
| Parking Brake | Hand Operate |
| Braking Type | Air Braking |
| Axle | With hub reducer |
| **Overall Weight** | 5800kg |
| **Tire Model** | 16/70-20, 16ply |
| **Max. Lifting Height** | 5140mm |
| **Rated Load** | 2500kg |
| **Transmission System** | Hydraulic Converter+Drive Shaft+Axles |
| **Driving Speed** | 18Km/H |
| **Wheelbase** | 2490mm |
| **Track** | 1470mm |
| **Ground Clearance** | 345mm |
| **Min Turning Radius** | 5600mm |
| **System Pressure** | 20Mpa |
| **Hydraulic output** | 104L/min |
| **Max. Height to the Pin** | 4650 mm |