DY25 Small Wheel Loader

**DY25 Optional Engines:**

****

|  |  |  |
| --- | --- | --- |
| **Engine Brand** | **Changchai 3M78** | **Kubota D1105** |
| **Emission Standard** | EURO V | EPA Tier 4 / Euro 5 |
| **Cooling System** | Water cooling | Water cooling |
| **Cylinders** | 3 Cylinders | 3 Cylinders |
| **Rated Power** | 17.65KW | 18.2KW |
| **R.P.M.** | 3000 r/min | 3000 r/min |

**DY25 Specifications:**

|  |  |
| --- | --- |
| **Items** | **Data** |
| Operating Weight (Without Attachment) | 1400kg |
| Max Travel Speed | 10km/h |
| Rated Operating Capacity(Bucket/Fork) | 809kg/527kg |
| Max.Lifting Height | 3400mm |
| Tipping Height | 1970mm |
| Wheel Base | 1345mm |
| Turn Radius (Inside) | 865mm |
| Turn Radius (Outside) | 2210mm |
| Max. Turn Radius | 1829mm |
| Bucket Capacity | 0.3-0.48m3 |
| Working Oil Flow | 33.6L/Min |
| Tracking Oil Flow | 78.4L/Min |
| Tires | 26X12-12, 8PLY |