DY35 Small Wheel Loader

**DY35 Optional Engines:**

****

|  |  |  |  |
| --- | --- | --- | --- |
| **Engine Brand** | **Changchai ZN390** | **Changchai ZN390** | **Kubota V1505-E4B** |
| Emission | Chinese stage III | Euro stage V | Euro stage V /  EPA Tier 4 |
| Cooling System | Water cooling | Water cooling | Water cooling |
| Cylinders | 3 Cylinders | 3 Cylinders | 3 Cylinders |
| Rated Power | 28.5KW | 18.5KW | 18.2KW（27.8HP） |
| R.P.M. | 2600r/min | 2400r/min | 2300 r/min |

**DY35 Specifications**

|  |  |
| --- | --- |
| **Items** | **Data** |
| Operating Weight (Without Attachment) | 2250kg |
| Max Travel Speed | 17km/h |
| Rated Operating Capacity (Bucket/Forks) | 1158kg/850kg |
| Max.Dump Height | 3717mm |
| Tipping Height | 2272mm |
| Wheel Base | 1502mm |
| Turn Radius (Inside) | 1106mm |
| Turn Radius (Outside) | 2625mm |
| Max. Turn Radius | 2206mm |
| Bucket Capacity | 0.3-0.48m3 |
| Working Oil Flow | 46.8L/Min |
| Tracking Oil Flow | 46.8L/Min |
| Tires | 31X15.5-15, 8PLY |