FL1000 Articulated Mini Loader

**FL1000 Optional Engines:**

****

|  |
| --- |
| **FL1000 Optional Engines** |
| **Engine Brand** | **Changchai 3M78** | **Kubota D1105** |
| **Emission Standard** | Euro V | EPA Tier 4 / Euro 5 |
| **Cooling System** | Water cooling | Water cooling |
| **Cylinders** | 3 Cylinders | 3 Cylinders |
| **Rated Power** | 17.65KW | 18.2KW |
| **R.P.M.** | 3000 r/min | 3000 r/min |

**FL1000 Specifications**

|  |  |
| --- | --- |
| **Model** | **FL1000** |
| Maximum Mast Height | 12ft=3.66 meters |
| Lifting Capacity(to Truck bed on level ground) | 1100kg |
| Total Weight | 1652kg |
| Max. Lifting height | 3000mm |
| Overall Length (without fork) | 2460mm |
| Ground Clearance | 22.86cm |
| Wheel Base | 1345mm |
| Frame Oscillation | ±8 degrees |
| Alternator | 12V, 360w |
| Standard Tires | 26X12-12, 8 Ply |
| Length of Forks | 1070mm |
| Dimensions (L\*W\*H) | 3900mm\*1230mm\*2186mm |
| Turn Radius (Inside) | 865mm |
| Turn Radius (Outside) | 2210mm |