
**DY620E Telescopic Wheel Loader**



TAIAN electric power mini loader, the DY620E, is a zero emission, low noise and hydrostatic telescopic wheel loader, it’s full-electric drive, battery-powered compact loader, which can perfect to replace fuel machine in multiple working area.

**DY620E Features:**





* Battery driven, 100% full electric;
* Lead-acid batteries;
* 300 Ah/12kWh battery capacity;
* External battery charger;
* No exhaust emissions;
* Low noise;
* Hydrostatic 4WD;
* Italian PWG brand drive motor;
* Auxiliary hydraulics oil flow max. 30L/min;
* 1 way hydraulic output with 1 electric output on the front;
* Hydraulic oil cooler;
* Telescopic boom;
* Handbrake parking brake;
* ROPS + FOPS canopy;
* 2 front &1 rear LED work lights;





**DY620E Specifications**

|  |  |
| --- | --- |
| **Model** | **DY620E** |
| **Overall Dimensions (L\*W\*H)** | 2390\*980\*1965mm |
| **Max. Reach (Boom Extended)** | 2750mm |
| **Max. Reach (Boom Retracted)** | 2220mm |
| **Rated Loading Capacity** | 500kg-800kg |
| **Min. Turning Radius** | 1980mm |
| **Turning Angle** | 400 |
| **Transmission** | 4WD / Hydrostatic |
| **Speed** | 8km/h |
| **Weight** | 1500 kg |
| **Standard Tire** | 23X8.5-12 |
| **Tire Pressure** | 2.8 bar |
| **Oil Tank Capacity** | 35L |
| **Working Pressure** | 180bar |
| **Working Oil Flow** | 30L/min |
| **Tracking pressure** | 230Bar |
| **Oil Model(mineral oil)** | L-HL46 |
| **Battery** | Lead-acid Battery capacity |
| **Battery Capacity** | 12 kWh/300Ah |
| **Power** | Electric |
| **Angle of Departure** | 25° |

**DY620E Dimensions**

****



**DY620E Optional Cabin****s:**

|  |  |
| --- | --- |
| **Steel Proof Canopy** | **Collapsible Roll Bar** |
| S0336036 | QQ图片20140929145532 |

**DY620E Optional Tires (23X8.5-12)**

|  |  |
| --- | --- |
| **Standard OTR Tire** | **Turf Tire** |
| IMG_256 |  |

**DY620E Other Options:**

|  |  |
| --- | --- |
| **Trailer hook** | **2 Way Multi Coupling Connectors\*** |
| IMG_0146 | **DY620 with 2 Way Multi Coupling System (11)** |

**\*The information and images in this document are provided for illustrative purpose only and do no bind the manufacturer, who reserves the right to make modifications at any time without prior warning.**

**REMARKS:**

**1.Payment:**30% T/T in advance, 70% T/T against the copy of B/L; Or irrevocable L/C at sight;

**2.Packing:**4 sets in 1\*20’GP, 8 sets in 1\*40’GP;

Or plywood box for 1 set (with additional package costs).

**3.Price Valid:**30 days.

**4.MOQ:**1SET.

**5.H.S. Code:**8429510005.

**6.Warranty:**1 year or 1000 working hours whichever comes first.

**\*2-Way Coupling Connectors:**

-Convenient and efficient coupling for hydraulic control attachments.

-Both the machine end and the attachments end need to install matching connectors.